	
	
	



[image: ]ONE WASHINGTON BLVD. 
DETROIT, MI 48226
PURCHASING DEPT. 
PHONE: (313) 877-8025 

HUNTINGTON PLACE CONVENTION CENTER - DETROIT 
** REQUEST FOR QUOTE** 
Please complete the following information to be considered for 
TRAILER JETTER RFQ 6.2627

DATE ISSUED:______09/04/2026_____	DUE DATE:______09/18/2026___________________
SEND RESPONSE TO:	DETROIT REGIONAL CONVENTION FACILITY AUTHORITY 
ONE WASHINGTON BLVD, DETROIT, MI 48226 
ATTN:  PURCHASING DIRECTOR 
PURCHASING@DRCFA.ORG 

*        *       *       *       *     *        *       *       *       *      *        *       *       *       *   *        *       *       *   *       *            
LOCATION OF SERVICES: 	HUNTINGTON PLACE CONVENTION CENTER 
ONE WASHINGTON BLVD, DETROIT, MI 48226 


DRCFA reserves the right to reject any and all quotations, to award to other than the low-cost respondent, and to request interviews from one, some, or none firms. DRCFA reserves the right to cancel any resulting Contract with notice at any time. DRCFA payment terms are net 30.  
Company Name: _________________________________________________________________
Address: _________________________________________________________________________
City, State, Zip:____________________________________________________________________
Contact Name and Title: ___________________________________________________________
Authorized Signature: ______________________________________________________________
Telephone: ___________________________ Email: ___________________________________
Indicate if SBE Firm:________________________________________________________________
Bidder to confirm that they can obtain parts on all equipment listed:     YES________ NO________

Quotation must include all applicable charges. DRCFA is not responsible for any charges not listed in this quotation. There shall not be any other charges if awarded a contract (ie fuel surcharge, mileage, hotel, etc) for any reason.

BIDDER TO INCLUDE REQUIRED DOCUMENTS: 
1. Warranties/Guarantees
2. This RFQ form

SPECS
· Pipe sizes: 3" - 12"diameter
· Pressure 3,000 PSE
· Flow: 12 GPM
· Standard hoses: 350’ of 3/8" high-pressure cleaning hose; 100’ of 5/8” rubber supply hose: 75’ of 1/4"
· trap-cleaning hose
· Weight: 1,260 lbs empty: 2,440 Ibs full 
· Size:120’W x 58” H x 53'D
· Engine: 45.5 cu in (747 cc) twin-cylinder, air cooled EFl engine with electric start and electronic ignition
· Nozzles included: one penetrator and one closed stainless steel nozzle


	Item Number
	Description
	Quantity
	Unit Price
	Extended Price

	
	758 EFI Trailer, 350’ HOSE
	
	
	

	
	Nozzle Kit, 3000 PSI
	
	
	

	
	Hose, S.S. TRAP 75’ LG
	
	
	

	
	
	
	
	

	Subtotal
	

	Sales Tax
	

	Shipping & Handling
	

	GRAND TOTAL 
	


**Sales Tax Exempt form issued upon request
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